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Dale Electric | Open Type Diesel Generator Set | 110 kVA ESP | Year of Manufacture 1972
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General Information
Low hours 110 kVA 100 kVA PRP Dale diesel generator set built on skids
Our Ref: FWP697    
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Key Specifications: 
Engine: DaleDimensions: 
· Length: TBC mm
· Width:   TBC mm
· Hight:    TBC mm 
· Weight: TBC kg
· Fuel Tank: N/A


Alternator: Dale
Frequency: 50 Hz
Speed: 1500 RPM
Voltage: 400/230V
Power: 100 kVA /88 kW | 153 Amps
Year: 1972
Hours: TBC 
Canopy Type: Open
Control Panel: Analog  

Control & Distribution:
This is a vintage used industrial generator in unrestored condition. It shows age-related wear, paint deterioration and areas of surface corrosion, as clearly shown in the photographs.

Highlights:
• Low hours (Fully 75 point checked and approved)
• Good Condition
• Ready for immediate deployment
MORE PHOTOS BELOW 
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FW Power Generators Ltd 
Phone: 01829 863497 | Email: info@fwpower.co.uk | www.fwpower.co.uk 
UK Company Registration Number: 15932066
UK VAT No: 480 3826 83 
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